SAS CONTROL MODULE REMOVAL/INSTALLATION

#
SAS CONTROL MODULE REMOVAL/INSTALLATION

B3E081057030W01

  Warning

  • Handling the SAS control module improperly can accidentally deploy the air bag modules and pre-tensioner seat belt, which may seriously injure you. Read the service warnings and cautions before handling the air bag module. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.)

  Caution

  • Handling the SAS control module improperly can accidentally deploy the air bag modules and pre-tensioner seat belt, which may seriously injure you. If configuration is not completed before removing the SAS control module, DTC B2477 will be displayed.

1. Perform SAS control module configuration when replacing it. (See SAS CONTROL MODULE CONFIGURATIONS.)

2. Turn the ignition switch to the LOCK position.

3. Disconnect the negative battery cable and wait for 1 min or more.

4. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

1 | Connector
2 | Bolt
3 | SAS control module

6. Install in the reverse order of removal.

7. Turn the ignition switch to the ON position.

  • If the SAS control module is replaced, turn the ignition switch to the ON position for 20 s or more after completing the configuration.

8. Verify that the air bag system warning light illuminates for approx. 6 s and goes out.

  • If the air bag system warning light does not operate normally, refer to the on-board diagnostic system (air bag system) and perform inspection of the system.