DTC 07:ER07

#
DTC 07:ER07

B3E090266900W22

DTC 07:Er07 | MD player

DETECTION CONDITION

  Note

  • When error occurs, error message "CHECK MD" is displayed in the LCD.

• Base unit detects MD reading error.

POSSIBLE CAUSE | • Defective MD (scratches or dirt) • MD player malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Verify the condition of the MD when the error occurs. Is the MD normal? | Yes | Go to the next step.
No | Repair (remove foreign material, clean) or replace the MD, and go to the next step.
2 | Clear the DTC, and then insert a normal MD. Play the MD for 12 s or more. Is DTC 07: Er07 displayed? | Yes | Replace the MD player.
No | DTC troubleshooting completed.