EGR VALVE REMOVAL/INSTALLATION [ZJ, Z6]

#
EGR VALVE REMOVAL/INSTALLATION [ZJ, Z6]

B3E011620300W02

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].)

2. Disconnect the negative battery cable.

3. Disconnect the EGR valve connector.

4. Remove in the order indicated in the table.

.

1 | EGR pipe (Exhaust manifold side) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [ZJ, Z6].)
2 | EGR valve

5. Install in the reverse order of removal.