SELECTOR LEVER COMPONENT INSPECTION

#
SELECTOR LEVER COMPONENT INSPECTION

B3E051846102W02

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)

2. Disconnect the negative battery cable.

3. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

4. Disconnect the selector lever component connector.

5. Verify that the continuity is as indicated in the table.

  • If there is any malfunction, adjust the selector cable. (See SELECTOR CABLE ADJUSTMENT.)