DRIVE SHAFT INSPECTION

#
DRIVE SHAFT INSPECTION

B3E031325500W02

1. Inspect the connections for any looseness.

  • If there is any malfunction, tighten or replace the applicable part.

2. Inspect the dust boot for damage and cracks.

  • If there is any malfunction, replace the applicable part.

3. Move the spline and joint up and down, left and right by hand and verify that there is no excessive play.

  • If there is any malfunction, replace the applicable part.