JOINT SHAFT DISASSEMBLY/ASSEMBLY

#
JOINT SHAFT DISASSEMBLY/ASSEMBLY

B3E031325700W03

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

.

1 | Joint shaft (See Joint Shaft Disassembly Note.) (See Joint Shaft Assembly Note.)
2 | Bearing (See Bearing Disassembly Note.) (See Bearing Assembly Note.)
3 | Dust seal (LH) (See Dust Seal (LH) Assembly Note.)
4 | Dust seal (RH) (See Dust Seal (RH) Assembly Note.)
5 | Bracket

## Joint Shaft Disassembly Note

1. Remove the joint shaft using a press.

## Bearing Disassembly Note

1. Remove the bearing and the dust seal (RH/LH) using the SSTs.

2. If the bearing remains on the joint shaft, set the SST and joint shaft to the press.

## Dust Seal (RH) Assembly Note

1. Apply grease to a new dust seal lip.

2. Install the dust seal (RH) using the SSTs.

## Bearing Assembly Note

1. Install a new bearing using the SSTs.

## Dust Seal (LH) Assembly Note

1. Apply grease to a new dust seal lip.

2. Install a new dust seal (LH) using the steel plate and the SSTs.

## Joint Shaft Assembly Note

1. Press fit the joint shaft using the SST and a press.