TRANSAXLE OIL INSPECTION [F35M-R]

#
TRANSAXLE OIL INSPECTION [F35M-R]

B3E051527001W01

1. Park the vehicle on level ground.

2. Remove the oil level plug and washer.

3. Verify that the oil level is as shown in the figure.

  • If the oil level is lower than the low level, add the specified amount and type of oil through the oil level plug hole.

  Oil grade
  API Service GL-4 or GL-5
  Oil viscosity
  All-season: SAE 75W-90
  Above 10 °C {50 °F}: SAE 80W-90

4. Install a new washer and the oil level plug.

  Tightening torque
  39-59 N·m {4.0-6.0 kgf·m, 29-43 ft·lbf}