PARKING BRAKE LEVER REMOVAL/INSTALLATION

#
PARKING BRAKE LEVER REMOVAL/INSTALLATION

B3E041244300W06

1. Remove the main silencer. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [ZJ, Z6].) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [LF].)

2. Remove the heat insulator.

3. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. After installation, inspect the parking brake lever stroke. (See PARKING BRAKE LEVER INSPECTION.)

.

1 | Parking brake switch connector
2 | Adjusting nut
3 | Parking brake lever
4 | Front parking brake cable (See Front Parking Brake Cable Installation Note.)
5 | Rear parking brake cable (See Rear Parking Brake Cable Installation Note.)

## Rear Parking Brake Cable Installation Note

1. Pass the rear parking brake cable inside the rear ABS wheel-speed sensor wiring harness as shown in the figure.

2. Install the rear parking brake cable.

## Front Parking Brake Cable Installation Note

1. Install the front parking brake cable with the mark on the equalizer facing toward the vehicle downside.