CLIMATE CONTROL UNIT REMOVAL [MANUAL AIR CONDITIONER]

#
CLIMATE CONTROL UNIT REMOVAL [MANUAL AIR CONDITIONER]

B3E074061190W02

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Ashtray panel (See CONSOLE REMOVAL/INSTALLATION.)
  (2) Detach the bonnet release lever from the lower panel. (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [L.H.D.].) (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [R.H.D.].)
  (3) Front scuff plate (SeeFRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (4) Front side trim (SeeFRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (5) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)
  (6) Front scuff plate (RH) (SeeFRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (7) Front side trim (RH) (SeeFRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (8) Decoration panel (SeeDECORATION PANEL REMOVAL/INSTALLATION.)
  (9) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)
  (10) PJB and PJB bracket (See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.)

3. Detach the PJB wiring harness clamp from the dashboard.

4. Remove the center panel module. (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)

5. Remove the air intake wire, air mix wire and airflow mode wire from the A/C unit.

6. Release the left and right tabs and remove in the order indicated in the table.

1 | Screw
2 | Fan switch connector
3 | Climate control unit connector
4 | Climate control unit