DTC C1145, C1155, C1165, C1175 [DSC]

#
DTC C1145, C1155, C1165, C1175 [DSC]

B3E040243000W19

DTC | C1145, C1155, C1165, C1175 | ABS wheel-speed sensor
DETECTION CONDITION | • Open circuit or short to ground has been detected in the ABS wheel-speed sensor wiring harness on any of the four vehicle wheels.

POSSIBLE CAUSE

• Open circuit or short to ground in the wiring harness between the following DSC HU/CM terminals and the ABS wheel-speed sensor terminals:

  - DSC HU/CM terminal AP-RF ABS wheel-speed sensor terminal A
  - DSC HU/CM terminal AS-RF ABS wheel-speed sensor terminal B
  - DSC HU/CM terminal I-LF ABS wheel-speed sensor terminal A
  - DSC HU/CM terminal F-LF ABS wheel-speed sensor terminal B
  - DSC HU/CM terminal O-RR ABS wheel-speed sensor terminal A
  - DSC HU/CM terminal R-RR ABS wheel-speed sensor terminal B
  - DSC HU/CM terminal AJ-LR ABS wheel-speed sensor terminal A
  - DSC HU/CM terminal AG-LR ABS wheel-speed sensor terminal B

• ABS wheel-speed sensor malfunction
• Poor connection at connectors (female terminal)

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---

1

INSPECT ABS WHEEL-SPEED SENSOR FOR SHORT TO GROUND
• Turn the ignition switch off.
• Disconnect the DSC HU/CM connectors.
• Inspect for continuity between the following DSC HU/CM connector terminals (vehicle harness-side) and body ground:

  - RF ABS wheel-speed sensor(+): AP
  - RF ABS wheel-speed sensor(-): AS
  - LF ABS wheel-speed sensor(+): I
  - LF ABS wheel-speed sensor(-): F
  - RR ABS wheel-speed sensor(+): O
  - RR ABS wheel-speed sensor(-): R
  - LR ABS wheel-speed sensor(+): AJ
  - LR ABS wheel-speed sensor(-): AG

• Is there continuity?

Yes

Go to the next step.

No | Go to Step 3.

2

INSPECT ABS WHEEL-SPEED SENSOR WIRING HARNESS FOR SHORT TO GROUND
• Disconnect the ABS wheel-speed sensor connectors.
• Inspect for continuity between the following DSC HU/CM connector terminals (vehicle harness-side) and body ground:

  - RF ABS wheel-speed sensor(+): AP
  - RF ABS wheel-speed sensor(-): AS
  - LF ABS wheel-speed sensor(+): I
  - LF ABS wheel-speed sensor(-): F
  - RR ABS wheel-speed sensor(+): O
  - RR ABS wheel-speed sensor(-): R
  - LR ABS wheel-speed sensor(+): AJ
  - LR ABS wheel-speed sensor(-): AG

• Is there continuity?

Yes

Repair or replace the wiring harness, then go to Step 4.

No | Replace the ABS wheel-speed sensor, then go to Step 4. (See FRONT ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION.) (See REAR ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION.)

3

INSPECT ABS WHEEL-SPEED SENSOR WIRING HARNESS FOR OPEN CIRCUIT
• Inspect for continuity between the DSC HU/CM connectors (vehicle harness-side) and the following vehicle harness-side terminals of ABS wheel-speed sensors:

  - RF ABS wheel-speed sensor(+): AP-A
  - RF ABS wheel-speed sensor(-): AS-B
  - LF ABS wheel-speed sensor(+): I-A
  - LF ABS wheel-speed sensor(-): F-B
  - RR ABS wheel-speed sensor(+): O-A
  - RR ABS wheel-speed sensor(-): R-B
  - LR ABS wheel-speed sensor(+): AJ-A
  - LR ABS wheel-speed sensor(-): AG-B

• Is there continuity?

Yes

Go to the next step.

No | Replace the ABS wheel-speed sensor, then go to the next step. (See FRONT ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION.) (See REAR ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION.)
4 | VERIFY THAT THE SAME DTC IS NOT PRESENT • Reconnect all disconnected connectors. • Clear the DTCs from the memory. (See Clearing DTCs Procedures.) • Are the same DTCs present? | Yes | Repeat the inspection from Step 1. If the malfunction recurs, replace the DSC HU/CM, then go to the next step. (See DSC HU/CM REMOVAL/INSTALLATION.)
No | Go to the next step.
5 | VERIFY THAT NO OTHER DTCS ARE PRESENT • Are any other DTCs output? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | DTC troubleshooting completed.