REAR LATERAL LINK REMOVAL/INSTALLATION

#
REAR LATERAL LINK REMOVAL/INSTALLATION

B3E021428600W01

1. Remove the rear auto leveling sensor. (See AUTO LEVELING SENSOR REMOVAL/INSTALLATION.)

2. Remove the rear stabilizer. (See REAR STABILIZER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

5. Inspect the wheel alignment and adjust it if necessary.

(See REAR WHEEL ALIGNMENT.)

.

1 | Rear lower arm outer bolt (See Rear Lower Arm Outer Bolt Removal Note.)
2 | Rear coil spring component (See REAR COIL SPRING REMOVAL/INSTALLATION.)
3 | Rear lateral link (See Rear Lateral Link Installation Note.)

## Rear Lower Arm Outer Bolt Removal Note

1. Support the rear lower arm using a jack.

2. Loosen the rear lower arm inner bolt.

3. Remove the rear lower arm outer bolt.

## Rear Lateral Link Installation Note

1. Install the rear lateral link so that the rib is facing toward the front of the vehicle.