IGNITION COIL REMOVAL/INSTALLATION [ZJ, Z6]

#
IGNITION COIL REMOVAL/INSTALLATION [ZJ, Z6]

B3E011801009W03

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].)

2. Disconnect the negative battery cable.

3. Remove the air cleaner (L.H.D.). (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [ZJ, Z6].)

4. Set the air cleaner cover out of the way (R.H.D.).

5. Remove the air cleaner case (R.H.D.). (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [ZJ, Z6].)

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

.

1 | Connector
2 | Ignition coil