THERMOSTAT REMOVAL/INSTALLATION [LF]

#
THERMOSTAT REMOVAL/INSTALLATION [LF]

B3E011215171W02

  Warning

  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [LF].)

2. Disconnect the negative battery cable.

3. Remove the under cover and splash shield as a single unit.

4. Drain the engine coolant. (See ENGINE COOLANT REPLACEMENT.)

5. Set the coolant reserve tank out of the way.

6. Remove the plug hole plate. (See PLUG HOLE PLATE REMOVAL/INSTALLATION [LF].)

7. Set the drive belt out of the way. (See DRIVE BELT REPLACEMENT [LF].)

8. Remove the drive belt tensioner. (See TIMING CHAIN REMOVAL/INSTALLATION [LF].)

9. Remove in the order indicated in the table.

10. Install in the reverse order of removal.

11. Add engine coolant. (See ENGINE COOLANT REPLACEMENT.)

12. Inspect for the engine coolant leakage. (See ENGINE COOLANT LEAKAGE INSPECTION.)

1 | Heater hose
2 | Lower radiator hose
3 | Thermostat component
4 | Gasket