#
TURBINE SENSOR REMOVAL/INSTALLATION

BHE051319200W07

  Caution

  • Water or foreign material entering the connector can cause poor connections or corrosion. Be sure that water or foreign material do not enter the connector when disconnecting it.
  • If foreign material is stuck to the turbine sensor, disturbance by magnetic flux can cause sensor output to be abnormal and there by negatively affect control. Make sure that foreign material such as iron particles is not stuck to the turbine sensor during installation.

1. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)

2. Remove the battery cover.

3. Disconnect the negative battery cable.

4. Remove the catalytic converter.

(See EXHAUST SYSTEM REMOVAL/INSTALLATION.)

5. Disconnect the turbine sensor connector.

6. Remove the turbine sensor.

7. Apply ATF to a new O-ring and install it on a turbine sensor.

8. Install the turbine sensor.

  Tightening torque
  5.0-7.0 N·m {51-71 kgf·cm, 43-61 in·lbf}

9. Connect the turbine sensor connector.

10. Install the catalytic converter.

(See EXHAUST SYSTEM REMOVAL/INSTALLATION.)

11. Connect the negative battery cable.

12. Install the battery cover.

13. Install the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)