#
RECLINER MOTOR INSPECTION

BHE091388663W01

1. Disconnect the recliner motor connector.

2. Connect battery positive voltage to recliner motor terminal A or B, then verify that the recliner motor operate as shown in the table.

  • If the recliner motor does not operate as indicated in the table, replace the recliner motor.

Motor operation | Connection
--- | ---
B+ | GND
Forward | A | B
Backward | B | A