#
CENTER SPEAKER REMOVAL/INSTALLATION

BHE092066961W07

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)
  (2) Console (See CONSOLE REMOVAL/INSTALLATION.)
  (3) Center panel module (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)
  (4) Center ventilator grille (See VENTILATOR GRILLE REMOVAL/INSTALLATION.)
  (5) LCD unit (See LCD UNIT REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Screw
2 | Center speaker
3 | Connector

4. Install in the reverse order of removal.