#
CENTER PANEL MODULE REMOVAL/INSTALLATION

BHE092066900W01

1. Disconnect the negative battery cable.

2. Remove the lower panel.(See LOWER PANEL REMOVAL/INSTALLATION.)

3. Remove the ashtray panel. (See CONSOLE REMOVAL/INSTALLATION.)

4. Remove the ventilator grille (enter). (See VENTILATOR GRILLE REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

1 | Screw
2 | Bolt
3 | Center panel module (See Center Panel Module Removal Note.)
4 | Connector (See Connector Removal Note.)
5 | Antenna feeder

6. Install in the reverse order of removal.

  Caution

  • When installing the center panel module, make sure that the wiring harness and antenna feeder are not caught between the unit and dashboard.If the wiring harness or the antenna feeder is caught between the unit and dashboard, it may cause malfunctions.

## Center Panel Module Removal Note

1. Pull the center panel module outward, detach clip A from the dashboard, and then remove the center panel module.

## Connector Removal Note

1. Put your hand through the opening where the ventilator grille was removed and disconnect the connectors.

  Caution

  • When putting your hand through the opening, be careful not to contact the panel edge or sharp parts to avoid injury.