#
HEADLIGHT CLEANER MOTOR INSPECTION

BHE091966122W06

1. Disconnect the negative battery cable.

2. Remove the windshield washer tank. (See WINDSHIELD WASHER TANK REMOVAL/INSTALLATION.)

3. Connect battery positive voltage to headlight cleaner motor terminal A and terminal B to ground.

4. Verify that the headlight cleaner motor operates normally.

  • If there is any malfunction, replace the headlight cleaner motor.