#
PILOT BEARING INSPECTION/REPLACEMENT [MT]

BHE011011D01E03

## Inspection

  Caution

  • Inspect the pilot bearing when it is installed to the eccentric shaft.

1. Before removing the pilot bearing, inspect it for damage, wear, and proper rotation.

  • If there is any malfunction, replace the pilot bearing.

## Replacement

### Removal

1. Fix the eccentric shaft on a vice.

2. Remove the pilot bearing and the oil seal together using the SST.

### Installation

1. Install a new pilot bearing using the SSTs.

2. Apply grease to the pilot bearing.

3. Install a new oil seal using the SSTs.