#
HVAC SPECIFICATIONS [MANUAL AIR CONDITIONER]

BHE070001038T04

## Basic System

Item | Specification
--- | ---
Heating capacity | (kW {kcal/h}) | 4.400 {3,784}
Cooling capacity | (kW {kcal/h}) | 4.500 {3,870}
Refrigerant | Type | R-134a
Regular amount (approx. quantity) | (g {oz}) | 430 {15.2}
A/C compressor | Type | Scroll type
Discharge capacity | (ml {cc, fl oz}) | 60 {60, 2.03}
Max. allowable speed | (rpm) | 9,000
Lube oil | Type | DENSO OIL8
Sealed volume (approx. quantity) | (ml {cc, fl oz}) | 60 {60, 2.03}
Condenser | Type | Multiflow (sub-cooling type)
Radiated heat | (kW {kcal/h}) | 7.0 {6,020}
Receiver/drier capacity | (ml {cc, fl oz}) | 190 {190, 6.42}
Desiccant | XH-9
Expansion valve | Type | External pressure equalizer
Evaporator | Type | Double-tank drawn cup
Temperature control | Reheat full air mix type

## Control System

Item | Specification
--- | ---
Airflow volume (during heater operation) | Blower motor | (m3/h) | 300
Electricity consumption (during heater operation) | Blower motor | (W) | 220
Airflow volume (during air conditioner operation) | Blower motor | (m3/h) | 460
Electricity consumption (during air conditioner operation) | Blower motor | (W) | 220
Magnetic clutch | (W) | 35
Magnetic clutch clearance | (mm {in}) | 0.20-0.45 {0.008-0.017}
Fan type | Blower motor | Sirocco fan
Refrigerant pressure switch | Type | Triple-pressure
Operating pressure |
(MPa {kgf/cm2, psi})
Sensor | Ambient temperature sensor | Thermistor
Evaporator temperature sensor
Actuator | Air intake actuator | Sliding contact type
Air mix actuator | Potentiometer type
Airflow mode actuator