#
REAR TRAILING LINK (LOWER) REMOVAL/INSTALLATION

BHE021428200W03

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. Inspect the rear wheel alignment.

(See REAR WHEEL ALIGNMENT.)

1 | Parking brake cable
2 | Caliper component (See Caliper Component Removal Note.)
3 | Disc plate
4 | Toe control link outer bolt
5 | Rear trailing link (lower) (See Rear Trailing Link (Lower) Removal Note.)

## Caliper Component Removal Note

1. Hang the caliper component and move aside.

## Rear Trailing Link (Lower) Removal Note

1. Support the rear knuckle using a jack.

  Caution

  • Be sure that the rear axle component is firmly supported by the jack. If not securely supported, the rear axle component could fall, resulting in serious injury or death, and damage to the vehicle.

2. Remove the rear trailing link (lower) outer bolt.

3. Remove the rear trailing link (lower) inner bolt.