#
DIFFERENTIAL OIL REPLACEMENT

BHE031427000W02

1. Position the vehicle on level ground.

2. Remove the oil-fill plug.

3. Remove the drain plug and drain the oil.

4. Install the drain plug with a new washer and tighten.

  Tightening torque
  39.2-53.9 N·m
  {4.00-5.49 kgf·m, 29.0-39.7 ft·lbf}

5. Add the specified oil through the oil-fill plug hole.

  Specified oil
  Type: API service GL-5
  Viscosity: SAE 90
  Oil capacity (approx. quantity):
  1.2-1.4 L
  {1.3- 1.4 US qt, 1.1-1.2 Imp qt}

6. After adding the oil, perform the oil level inspection.

7. Install the oil-fill plug with a new washer and tighten.

  Tightening torque
  39.2-53.9 N·m
  {4.00-5.49 kgf·m, 29.0-39.7 ft·lbf}