#
DISCHARGE HEADLIGHT CONTROL UNIT REMOVAL/INSTALLATION

BHE091851030W03

  Warning

  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the discharge headlight service warnings. (See DISCHARGE HEADLIGHT SERVICE WARNINGS.)

1. Disconnect the negative battery cable.

2. Remove the front side turn lights. (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Remove the front combination lights. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

5. Remove screws A, then remove the cover.

6. Disconnect the connector.

7. Remove screws B, then remove the discharge headlight control unit.

8. Install in the reverse order of removal.