#
RADIATOR SHROUD LOWER PANEL INSTALLATION

BHE098053100B04

1. Weld the 14 locations indicated by (A), then temporarily install the condenser bracket and oil cooler bracket.

2. When installing new parts, position each part so that the section measurement aligns with the body dimension.

3. Drill holes for plug welds before installing new parts.

4. Weld the remaining weld locations and install the radiator shroud lower panel.

5. After temporarily installing new parts, make sure the related parts fit properly.

  Note

  • When replacing the radiator shroud side stay and the bonnet lock bracket separately, weld the 27 locations indicated by (B).