#
DTC P0335

BHE010200300W05

DTC P0335 | Eccentric shaft position sensor circuit problem
--- | ---
DETECTION CONDITION | • The PCM monitors the input signal from the eccentric shaft position sensor when the mass intake airflow amount is more than 2 g/s {0.26 lb/min}. If the input signal is not input, the PCM determines that there is a eccentric shaft position sensor circuit malfunction. Diagnostic support note • This is a continuous monitor (CCM). • The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle. • PENDING CODE is available if the PCM detects the above malfunction condition. • FREEZE FRAME DATA is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Eccentric shaft position sensor malfunction • Connector or terminal malfunction • Open circuit in wiring harness between eccentric shaft position sensor terminal A and PCM terminal 2U • Short to power supply in wiring harness between eccentric shaft position sensor terminal A and PCM terminal 2U • Short to GND in wiring harness between eccentric shaft position sensor terminal A and PCM terminal 2U • Open circuit in wiring harness between eccentric shaft position sensor terminal B and PCM terminal 2X • Short to power supply in wiring harness between eccentric shaft position sensor terminal B and PCM terminal 2X • Short to GND in wiring harness between eccentric shaft position sensor terminal B and PCM terminal 2X • Eccentric shaft position sensor is dirty • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT ECCENTRIC SHAFT POSITION SENSOR CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the eccentric shaft position sensor connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
4 | INSPECT ECCENTRIC SHAFT POSITION SENSOR CIRCUIT FOR SHORT TO GND • Turn the ignition switch off. • Inspect for continuity between the following circuits: – Eccentric shaft position sensor terminal A (wiring harness-side) and body GND – Eccentric shaft position sensor terminal B (wiring harness-side) and body GND • Is there continuity? | Yes | Repair or replace the wiring harness for a possible short to GND, then go to Step 9.
No | Go to the next step.
5 | INSPECT ECCENTRIC SHAFT POSITION SENSOR CIRCUIT FOR SHORT TO POWER SUPPLY • Turn the ignition switch to the ON position (Engine off). • Measure the voltage between the following circuits: – Eccentric shaft position sensor terminal A (wiring harness-side) and body GND – Eccentric shaft position sensor terminal B (wiring harness-side) and body GND • Is the voltage B+? | Yes | Repair or replace the wiring harness for a possible short to power supply, then go to Step 9.
No | Go to the next step.
6 | INSPECT ECCENTRIC SHAFT POSITION SENSOR • Inspect the eccentric shaft position sensor. (See ECCENTRIC SHAFT POSITION SENSOR INSPECTION.) • Is there any malfunction? | Yes | Replace the eccentric shaft position sensor, then go to Step 9. (See ECCENTRIC SHAFT POSITION SENSOR REMOVAL/INSTALLATION.)
No | Go to the next step.
7 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
8 | INSPECT ECCENTRIC SHAFT POSITION SENSOR CIRCUIT FOR OPEN CIRCUIT • Turn the ignition switch off. • Inspect for continuity between the following circuits: – Eccentric shaft position sensor terminal A (wiring harness-side) and PCM terminal 2U (wiring harness-side) – Eccentric shaft position sensor terminal B (wiring harness-side) and PCM terminal 2X (wiring harness-side) • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for a possible open circuit, then go to the next step.
9 | VERIFY TROUBLESHOOTING OF DTC P0335 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine and run the engine for 5 s or more. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION.)
No | Go to the next step.
10 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE.) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE.)
No | DTC troubleshooting completed.