#
EVAPORATIVE CHAMBER INSPECTION

BHE011642590W01

1. Remove the rear differential. (See REAR DIFFERENTIAL REMOVAL/INSTALLATION.)

2. Remove the evaporative chamber installed on outside air side of the charcoal canister hose.

3. Blow air from port A using your mouth and verify that there is air flow.

  • If there is no air flow, replace the evaporative chamber.

4. Verify that there is no deformation or cracking of the evaporative chamber.

  • If the exterior is not normal, replace the evaporative chamber.