#
FAN MOTOR INSPECTION

BHE011215140W02

## Part inspection

1. Verify that the battery is fully charged.

2. Install a tester and battery to the cooling fan motor connector as shown in the figure.

3. Verify that each fan motor operates smoothly at the standard current.

  • If there is any malfunction, replace the applicable part.

Item | Current (A) [12V]
--- | ---
Cooling fan No.1 | 8.9-11.9
Cooling fan No.2 | 4.0-7.0