#
WINDSHIELD WIPER AND WASHER SWITCH INSPECTION

BHE091966122W04

1. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

2. Remove the ignition key illumination. (See IGNITION KEY ILLUMINATION BULB REMOVAL/INSTALLATION.)

3. Remove the windshield wiper and washer switch. (See WINDSHIELD WIPER AND WASHER SWITCH REMOVAL/INSTALLATION.)

4. Verify that the continuity between the windshield wiper and washer switch is as indicated in the table.

  • If not as indicated in the table, replace the windshield wiper and washer switch.