#
STEERING SHAFT INSPECTION

BHE061332100W01

1. Inspect the column bearing for excessive play and damage.

2. Verify that the measurement of the steering shaft is as specified in the figure.

  • If not within the specification, replace the steering shaft component.

  Standard
  508.5 mm {20.02 in}

3. Inspect the tilt function operation for the following.

  (1) Verify that the tilt lever moves smoothly from the lock to the unlock position.
  (2) Verify that the steering shaft is fixed firmly when the tilt lever is locked.

  • If there is any malfunction, replace the steering shaft.