#
PANEL LIGHT CONTROL SWITCH REMOVAL/INSTALLATION

BHE091866600W01

1. Disconnect the negative battery cable.

2. Remove the panel light control switch. (See Panel Light Control Switch Removal Note.)

3. Disconnect the connector.

4. Install in the reverse order of removal.

## Panel Light Control Switch Removal Note

1. Reach into the dashboard through the underside of the lower panel and, while pushing on the tabs of the panel light control switch, pull it outward.