#
ROTOR BEARING REPLACEMENT

BHE011011B10E08

## Removal

1. Set the rotor with the internal gear at the bottom.

2. Remove the adapter ring and the securing screw from the SST.

3. Remove the rotor bearing using the SST.

## Installation

1. Remove the SST handle.

2. Temporarily assemble so that the rotor bearing tab and the rotor notch are aligned after pressing in the rotor bearing and rotor.

3. Set the temporarily assembled rotor bearing and rotor on a hydraulic press.

4. Press in the rotor bearing using the SST.