#
WINDSHIELD WASHER NOZZLE REMOVAL/INSTALLATION

BHE091967510W01

1. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

2. Remove the windshield washer hose from the windshield washer nozzle. (See WINDSHIELD WASHER HOSE REMOVAL/INSTALLATION.)

3. Squeeze the tabs of the windshield washer nozzle.

4. Pull the windshield washer nozzle out to remove it.

5. Install in the reverse order of removal.