#
OIL COOLER REMOVAL/INSTALLATION

BHE011110040W01

  Warning

  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.

1. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION.)

4. Remove the following.

  (1) Front tire (LH)
  (2) Front tire (RH) (with twin oil cooler)
  (3) Under cover
  (4) Splash shield

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

7. Add engine oil. (See ENGINE OIL REPLACEMENT.)

8. Start the engine and confirm that there is no oil leakage from areas worked on.

  • If there is any oil leakage, find the cause and repair or replace the applicable part.

9. Inspect the oil level. (See ENGINE OIL LEVEL INSPECTION.)

1 | Oil cooler hose (See Oil Cooler Hose Removal Note)
2 | Oil cooler bracket
3 | Oil cooler
4 | Oil cooler duct

## Oil Cooler Hose Removal Note

  Note

  • Use a drain pan to catch the oil when the oil hoses are disconnected.