#
SIMULATION FUNCTION

BHE050201026T08

• By using the WDS or equivalent, simulation items for input/output parts preset in the TCM can be optionally selected and operated regardless of TCM control conditions.

## Simulation Item Table

X: Available

Simulation item | Applicable component | Unit/Condition | Operation | TCM terminal
--- | --- | --- | --- | ---
IG ON | Idle
24B_Duty | Shift solenoid valve B (2-4 brake duty) | % | X | X | 2S
HC_Duty | Shift solenoid valve C (high clutch duty) | % | X | X | 2V
LRB_Duty | Shift solenoid valve F (low and reverse brake duty) | % | X | X | 2P
LU_Duty | TCC solenoid valve (TCC solenoid duty) | % | X | X | 2W
PCSV | Pressure control solenoid valve | ON/OFF | X | X | 2X
TCCC | Shift solenoid valve A (low clutch duty) | % | X | X | 2Y