#
REAR HEAT DUCT REMOVAL/INSTALLATION

BHE071161273W01

1. Remove the following parts:

  1. Front seat (See FRONT SEAT REMOVAL/INSTALLATION.)
  2. Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  3. Inner scuff plate (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)
  4. Ashtray illumination bulb (See ASHTRAY ILLUMINATION BULB REMOVAL/INSTALLATION.)
  5. Console (See CONSOLE REMOVAL/INSTALLATION.)
  6. Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)
  7. Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  8. Seat belt rail (See FRONT SEAT BELT REMOVAL/INSTALLATION.)
  9. Floor covering (See FLOOR COVERING REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

1 | Rear heat duct (LH)
2 | Rear heat duct (RH)

3. Install in the reverse order of removal.