#
BATTERY REMOVAL/INSTALLATION

BHE011718520W01

  Warning

  • For vehicles with DSC, if the negative battery cable is disconnected, the stored initial position of the steering angle sensor will be cleared and the DSC will not operate properly, making the vehicle unsafe to drive. Perform the steering angle sensor initialization procedure after connecting the negative battery cable.

1. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

1 | Battery cover (See Battery Cover Removal Note.)
2 | Negative battery cable
3 | Positive battery cable
4 | Battery clamp
5 | Battery (See Battery Installation Note.)
6 | Battery box
7 | Battery tray
8 | Battery duct

3. Install in the reverse order of removal.

4. Perform the steering angle sensor initializtion procedure. (See STEERING ANGLE SENSOR INITIALIZATION PROCEDURE.)

## Battery Cover Removal Note

1. Pull up the two tabs on the rear, remove the tab on the front, and then remove the battery cover.

## Battery Installation Note

1. Install the 50D20L battery within the area of the white paint mark on the battery box.