#
ENTERTAINMENT OUTLINE

BHE092001066T01

• The center panel module installed with the audio unit and the audio switch, A/C switch, hazard warning switch and rear window defroster switch built into the center panel has been adopted.

• The audio unit consists of the following parts:

  – Base unit, which has AM/FM tuner and control function for each module
  – Upper module (CD player or CD changer)
  – Lower module (cassette deck or MD player)
  – Cover

• Upper module (CD player or CD changer) and lower module (cassette deck or MD player) are options.

• Module availability depends on vehicle grade.

• The audio control switch is equipped on the steering wheel for audio operation.

• The glass antenna has been adopted.

• The following speakers have been adopted for standard specification vehicles (4 speakers: European (L.H.D. U.K.) specs.) (6 speakers: Australian specs.):

  – Front door speaker
  – Rear speaker
  – Front tweeter (Australian specs.)

• The following speakers have been adopted for BOSE specification vehicles (9 speakers):

  – Front door speaker
  – Rear speaker
  – Front tweeter
  – Rear tweeter
  – Center speaker

• The auto level control (ALC) function has been adopted. (Standard specification)

• The noise-response sound compensation system (AudioPilot*) has been adopted. (BOSE specification)

• A noise filter has been installed on the brake light, rear window defroster and circuit, and a condenser has been installed on the high-mount brake light and trunk compartment light circuit for improved noise reduction.

• All information related to the audio system appears on the information display's LCD.

  * :
"AudioPilot" is a registered trademark of Bose Corporation.