#
SHIFT CONTROL STRUCTURE

BHE051318901T04

## Features

• The TCM selects and determines the shift diagram based on the results of the range and driving mode judgements. Then, based on the shift diagram, the TCM sends signals to the duty-cycle type solenoid valves and the ON/OFF type solenoid valves, according to the VSS and the throttle opening signals, to perform shifting.

## Structure

System diagram

1 | TR switch
2 | TFT sensor
3 | Selector lever component
4 | M range switch
5 | Up switch
6 | Down switch
7 | Throttle opening signal
8 | Engine torque signal
9 | Cruise control signal
10 | Engine coolant temperature signal
11 | Throttle opening angle
12 | Brake switch
13 | Up/down signal
14 | Steering shift switch
15 | Shift solenoid F
16 | Shift solenoid B
17 | Shift solenoid C
18 | Shift solenoid A
19 | Vehicle speed