#
POWER WINDOW SUBSWITCH REMOVAL/INSTALLATION

BHE091266330W03

1. Disconnect the negative battery cable.

2. Using a flathead screwdriver wrapped with protective tape, pry up the rear of the switch panel and detach the clip.

3. Remove the switch panel from the front door trim keeping the tab from catching.

4. Disconnect the power window subswitch connector.

5. Remove the screws, then remove the power window subswitch.

6. Install in the reverse order of removal.