#
EXTRACTOR CHAMBER REMOVAL/INSTALLATION

BHE091651908W01

1. Remove the following parts:

  (1) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)
  (2) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)
  (3) Rear combination light (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)
  (4) Rear bumper (See REAR BUMPER REMOVAL/INSTALLATION.)

2. Detach clips A by squeezing them from inside the vehicle, and remove the extractor chamber from the body.

3. Install in the reverse order of removal.