#
GENERATOR CONTROL BLOCK DIAGRAM

BHE014000140T49

• The PCM determines the engine operation and electrical load conditions based on input signals, and controls energization time of the generator field coil.

1 | Generator (Terminal P: Stator coil)
2 | Battery positive voltage
3 | Eccentric shaft position sensor
4 | ECT sensor
5 | Vehicle speed signal (CAN signal)
6 | IAT sensor
7 | Brake switch No.1 (CAN signal)
8 | A/C amplifier (A/C switch signal)
9 | TCM (AT) (CAN SIGNAL)
10 | PCM
11 | Generator (Terminal D: Field coil)