#
FLOOR COVERING REMOVAL/INSTALLATION

BHE091768660W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front seat (See FRONT SEAT REMOVAL/INSTALLATION.)
  (2) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (3) Inner scuff plate (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)
  (4) Ashtray illumination bulb (See ASHTRAY ILLUMINATION BULB REMOVAL/INSTALLATION.)
  (5) Console (See CONSOLE REMOVAL/INSTALLATION.)
  (6) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (7) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (8) Seat belt rail (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

3. Remove fasteners A, B, and C.

4. Detach clip D and remove the floor covering.

5. Take the floor covering out from the opened door.

6. Install in the reverse order of removal.