#
ECCENTRIC SHAFT BYPASS VALVE

BHE011011D01E04

  Warning

  • Engine oil temperature will increase during the inspection and become very dangerous. Be careful not to burn yourself during the inspection.

1. Put the eccentric shaft bypass valve in a container filled with engine oil.

2. Heat the container and verify that the projection protrudes more than the minimum specification when the engine oil temperature is 60 °C {140 °F}.

  • If it is less than the minimum specification, replace the eccentric shaft bypass valve.

  Minimum projection
  6 mm {0.24 in}