#
BLOWER UNIT DISASSEMBLY/ASSEMBLY

BHE071161140W02

1. Disassemble in the order indicated in the table.

  Caution

  • If a non-specified grease is used, it may result in abnormal noise or improper operation of the links. Apply only the specified grease to each link.

1 | Air filter cover
2 | Air filter
3 | Blower motor
4 | Air intake actuator
5 | Air intake link
6 | Plate
7 | Air intake door
8 | Adhesive polyurethane
9 | Blower case (1)
10 | Blower case (2)

2. Assemble in the reverse order of disassembly.