#
REFRIGERANT PRESSURE SWITCH REMOVAL/INSTALLATION

BHE074061503W01

1. Disconnect the negative battery cable.

2. Discharge the refrigerant from the system. (See REFRIGERANT CHARGING.)

3. Hold the piping block with pliers or a similar tool and loosen the refrigerant pressure switch using a wrench.

4. Remove in the order indicated in the table.

1 | Refrigerant pressure switch connector
2 | Refrigerant pressure switch (See Refrigerant Pressure Switch Installation Note.)

5. Install in the reverse order of removal.

## Refrigerant Pressure Switch Installation Note

1. Apply compressor oil to the O-ring joints.