#
MEMORY CLEARING PROCEDURE

BHE090266900W03

1. Start the on-board diagnostic test mode.

2. While pressing the POWER button, simultaneously press the AUDIO CONT button for 2 s or more.

1 | AUDIO CONT button
2 | POWER button

  Caution

  • Before clearing the memory, be sure to enter all of the DTCs displayed in the on-board diagnostic test mode in the Audio Repair Order Form.

3. To stop the on-board diagnostic test mode, turn the ignition switch to the LOCK position.