#
CONSOLE REMOVAL/INSTALLATION

BHE091764271W01

1. Disconnect the negative battery cable.

2. Detach clips A and remove the upper panel.

3. Disassemble in the order indicated in the table.

1 | Screw A
2 | Ashtray panel (SeeAshtray Panel Removal Note)
3 | Cigarette lighter connector
4 | Ashtray illumination (SeeASHTRAY ILLUMINATION BULB REMOVAL/INSTALLATION)
5 | Storage compartment
6 | Hole cover
7 | Screw B
8 | Rear console
9 | Screw C
10 | Front console
11 | Screw D
12 | Under cover

4. Install in the reverse order of removal.

## Ashtray Panel Removal Note

1. Remove the ashtray panel using a flathead screwdriver wrapped with protective tape.