#
TRUNK COMPARTMENT LIGHT SWITCH INSPECTION

BHE091851440W02

  Note

  • The trunk compartment light switch is built into the trunk lock.

1. Remove the trunk lid trim. (See TRUNK LID TRIM REMOVAL/INSTALLATION.)

2. Disconnect the trunk compartment light switch connector.

3. Verify that the continuity between the trunk compartment light switch terminals is as indicated in the table.

  • If not as indicated in the table, replace the trunk lock.