#
COWL SIDE REINFORCEMENT INSTALLATION

BHE098053290B02

1. When installing new parts, position each part so that the section measurement aligns with the body dimension.

2. Drill holes for plug welds before installing new parts.

3. Weld the 18 locations indicated by (A), then temporarily installing the cowl side reinforcement inner and cowl side reinforcement.

4. After temporarily installing new parts, make sure the related parts fit properly.