#
CRUISE CONTROL SWITCH INSPECTION

BHE012066341W01

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Disconnect the audio control switch connector.

4. Inspect for resistance and continuity between cruise control switch terminals B-C using a tester.

  • If not as specified, replace the cruise control switch.

Switch condition | Resistance (ohm)
--- | ---
ON/OFF button pressed | Continuity
CANCEL button pressed | 117-123
SET/COAST button pressed | 666-694
RES/ACCEL button pressed | 2,156-2,244
No button pressed | No continuity